{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["封面","27","21","18"],"not_rendered":{"external_links":3,"defined_names":9},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封面","index":0,"n_rows":7,"n_cols":9,"rows_kept":7,"merged":[[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3]],"flags":["formulas_cached_only"]}
[]
[null,"桥梁体积重量参考数据："]
[null,"序号","名称",null,"数量","体积m³","单重Kg","总体积m³","总重Kg"]
[null,1,"27.432米桥",null,2,{"v":72.26398653999999,"d":"72.26"},{"v":38483.76000000001,"d":"38483.8"},{"v":144.52797307999998,"d":"144.5"},{"v":76967.52000000002,"d":"76968"}]
[null,2,"21.336米桥",null,2,{"v":55.55763444000001,"d":"55.56"},{"v":28264.359999999997,"d":"28264.4"},{"v":111.11526888000002,"d":"111.1"},{"v":56528.719999999994,"d":"56529"}]
[null,3,"18.288米桥",null,2,{"v":47.90814944,"d":"47.91"},{"v":24359.98,"d":"24360.0"},{"v":95.81629888,"d":"95.8"},{"v":48719.96,"d":"48720"}]
[null,"汇总:",null,null,6,null,null,{"v":351.45954084000005,"d":"351.5"},182216.2]

{"sheet":"27","index":1,"n_rows":53,"n_cols":13,"rows_kept":53,"merged":[[0,0,0,12],[1,0,2,0],[1,1,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,8],[1,9,2,9],[1,10,2,10],[3,0,4,0],[3,1,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,9,4,9],[5,1,5,2],[5,3,8,3],[6,1,6,2],[7,1,7,2],[8,0,9,0],[8,1,8,2],[8,5,9,5],[8,7,9,7],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[9,1,9,2],[10,1,10,2],[11,1,12,2],[11,3,12,3],[11,4,12,4],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,0,18,0],[17,1,17,2],[17,5,18,5],[17,7,18,7],[17,8,18,8],[17,9,18,9],[17,10,18,10],[17,11,18,11],[17,12,18,12],[18,1,18,2],[19,1,20,2],[19,3,20,3],[21,1,21,2],[22,1,22,2],[26,0,27,12],[28,0,29,0],[28,1,29,2],[28,3,29,3],[28,4,29,4],[28,5,29,5],[28,6,28,8],[28,9,29,9],[28,10,29,10],[30,0,31,0],[30,1,31,2],[30,3,31,3],[30,4,31,4],[30,5,31,5],[30,6,31,6],[30,9,31,9],[32,0,49,0],[32,1,32,2],[32,5,49,5],[32,7,49,7],[32,8,49,8],[32,9,49,9],[32,10,49,10],[32,11,49,11],[32,12,49,12],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2]],"flags":["formulas_cached_only"]}
["1座27.432米桥捆装件清单（总计2座）"]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
["1","桁架 Panel-standard",null,28,322,1,4,1291.94,1288,"3163*2350*620",{"v":4.608491,"d":"4.61"},{"v":4.608491,"d":"4.61"},{"v":1291.94,"d":"1291.9"}]
["2~3","桁架 Panel-standard",null,null,322,2,7,2257.94,2254,"3163*2350*980",{"v":7.284389,"d":"7.28"},{"v":14.568778,"d":"14.57"},{"v":4515.88,"d":"4515.9"}]
["4","桁架 Panel-standard",null,null,322,1,9,2901.94,2898,"3163*2350*1248",{"v":9.2764464,"d":"9.28"},{"v":9.2764464,"d":"9.28"},{"v":2901.94,"d":"2901.9"}]
["5","桁架 Panel-standard",null,null,322,1,1,3029.94,322,"3163*2350*1296",{"v":9.6332328,"d":"9.63"},{"v":9.6332328,"d":"9.63"},{"v":3029.94,"d":"3029.9"}]
[null,"高剪桁架 High shear panel",null,8,338,null,8,null,2704]
["6~9","加强弦杆 Chord Reinforcement",null,28,89,4,7,627,623,"3163*700*176",{"v":0.3896815999999999,"d":"0.39"},{"v":1.5587263999999996,"d":"1.56"},{"v":2508,"d":"2508.0"}]
["10","超宽道横梁(6.2米)ExtreTransom-6.2m",null,10,471.3,1,4,1916.2,1885.2,"6200*800*575",{"v":2.8520000000000003,"d":"2.85"},{"v":2.8520000000000003,"d":"2.85"},1916.2]
["11~12",{"$nulls":4},2,3,1436.9,1413.9,"6200*590*575",{"v":2.10335,"d":"2.10"},{"v":4.2067,"d":"4.21"},2873.8]
["13~14","水平支撑架TR Bracing Frame",null,18,57.4,2,9,518.1,516.6,"2376*700*560",{"v":0.931392,"d":"0.93"},{"v":1.862784,"d":"1.86"},1036.2]
["15~16","竖向支撑架TR Vertical Frame",null,16,37,2,8,297,296,"1776*400*560",{"v":0.39782400000000007,"d":"0.40"},{"v":0.7956480000000001,"d":"0.80"},{"v":594,"d":"594.0"}]
["17","抗风拉杆 Sway Brace",null,18,43,1,18,791,774,"5076*340*425",{"v":0.733482,"d":"0.73"},{"v":0.733482,"d":"0.73"},{"v":791,"d":"791.0"}]
["18","竖向风构 Vertical Brace",null,18,15,1,18,270.5,270,"3001*270*230",{"v":0.18636210000000003,"d":"0.19"},{"v":0.18636210000000003,"d":"0.19"},270.5]
["19~20","阴头端柱Post-End-Female",null,4,89,2,2,343.5,332,"2629*432*390",{"v":0.44293392000000004,"d":"0.44"},{"v":0.8858678400000001,"d":"0.89"},{"v":687,"d":"687.00"}]
[null,"阳头端柱Post-End-Male",null,4,77,null,2]
["21~24","桥面板166 Deck-166",null,36,395,4,7,2771.3,2765,"3040*1162*1050",{"v":3.709104,"d":"3.71"},{"v":14.836416,"d":"14.84"},{"v":11085.2,"d":"11085.20"}]
["25~26",{"$nulls":3},395,2,4,1586.3,1580,"3040*664*1050",{"v":2.119488,"d":"2.12"},{"v":4.238976,"d":"4.24"},{"v":3172.6,"d":"3172.60"}]
["27","路缘 Kerb",null,18,26,1,18,488.8,468,"3040*756*330",{"v":0.7584192,"d":"0.76"},{"v":0.7584192,"d":"0.76"},{"v":488.8,"d":"488.80"}]
["28","加隙板4.2m Deck Eob Filler4.2m",null,2,85,1,2,171.3,170,"4200*332*97",{"v":0.1352568,"d":"0.14"},{"v":0.1352568,"d":"0.14"},{"v":171.3,"d":"171.30"}]
[]
[]
[]
["1座27.432米桥装箱件清单（总计2座）"]
[]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
[29,"桁架销 Penal Pin",null,107,3,1,107,1149.46,1011.4599999999999,"1280*880*1000",{"v":1.1264,"d":"1.13"},{"v":1.1264,"d":"1.13"},{"v":1149.46,"d":"1149.5"}]
[null,"保险卡环 Safety Pin",null,107,0.03,null,107]
[null,"联系梁TR Tie Beam",null,4,5.3,null,4]
[null,"支座  Bearing",null,8,13.4,null,8]
[null,"支座板 Baseplate",null,8,13,null,8]
[null,"弦杆螺栓Chord  Reinforcement  Bolt",null,120,0.98,null,120]
[null,"加隙板螺栓Deck Eob Filler Bolt",null,17,0.35,null,17]
[null,"撑架螺栓 Brace Bolt",null,135,0.5,null,135]
[null,"螺纹板 Nut-Deck-Clamp",null,168,0.35,null,168]
[null,"横梁螺栓Transom Bolt",null,42,0.8,null,42]
[null,"地脚螺栓 螺母 平垫圈 Bastplate Bolt",null,17,2,null,17]
[null,"拉杆螺栓Swaybrace Bolt",null,38,0.6,null,38]
[null,"风构螺栓Vertical Brace Bolt",null,57,0.5,null,57]
[null,"螺母M24 NutM24",null,392,"/",null,392]
[null,"螺母M20 NutM20",null,95,"/",null,95]
[null,"弹垫20  Washer",null,168,"/",null,168]
[null,"桥面板螺栓 Deck Screw  ",null,151,0.35,null,151]
[null,"路缘螺栓 Kerb-Bolt",null,95,0.35,null,95]
[]
[{"$nulls":10},"单桥总重量",null,{"v":38483.76000000001,"d":"38483.8"}]
[{"$nulls":10},"单桥总体积",null,{"v":72.26398653999999,"d":"72.26"}]

{"sheet":"21","index":2,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,0,12],[1,0,2,0],[1,1,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,8],[1,9,2,9],[1,10,2,10],[3,0,4,0],[3,1,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,9,4,9],[5,1,5,2],[5,3,7,3],[6,1,6,2],[7,0,8,0],[7,1,7,2],[7,5,8,5],[7,7,8,7],[7,9,8,9],[7,10,8,10],[7,11,8,11],[7,12,8,12],[8,1,8,2],[9,1,9,2],[9,22,9,23],[9,35,9,36],[9,48,9,49],[9,61,9,62],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,0,15,0],[14,1,14,2],[14,5,15,5],[14,7,15,7],[14,8,15,8],[14,9,15,9],[14,10,15,10],[14,11,15,11],[14,12,15,12],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[20,0,21,12],[22,0,23,0],[22,1,23,2],[22,3,23,3],[22,4,23,4],[22,5,23,5],[22,6,22,8],[22,9,23,9],[22,10,23,10],[24,0,25,0],[24,1,25,2],[24,3,25,3],[24,4,25,4],[24,5,25,5],[24,6,25,6],[24,9,25,9],[26,0,43,0],[26,1,26,2],[26,5,43,5],[26,7,43,7],[26,8,43,8],[26,9,43,9],[26,10,43,10],[26,11,43,11],[26,12,43,12],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2]],"flags":["formulas_cached_only"]}
["1座21.336米桥捆装件清单（总计2座）"]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
["1","桁架 Panel-standard",null,20,322,1,5,1613.94,1610,"3163*2350*712",{"v":5.2923316,"d":"5.29"},{"v":5.2923316,"d":"5.29"},{"v":1613.94,"d":"1613.9"}]
["2~3","桁架 Panel-standard",null,null,322,2,7,2257.94,2254,"3163*2350*980",{"v":7.284389,"d":"7.28"},{"v":14.568778,"d":"14.57"},{"v":4515.88,"d":"4515.9"}]
["4","桁架 Panel-standard",null,null,322,1,1,3029.94,322,"3163*2350*1296",{"v":9.6332328,"d":"9.63"},{"v":9.6332328,"d":"9.63"},{"v":3029.94,"d":"3029.9"}]
[null,"高剪桁架 High shear panel",null,8,338,null,8,null,2704]
["5~6","超宽道横梁(6.2米)ExtreTransom-6.2m",null,8,471.3,2,4,1916.2,1885.2,"6200*800*575",{"v":2.8520000000000003,"d":"2.85"},{"v":5.704000000000001,"d":"5.70"},3832.4]
["7","水平支撑架TR Bracing Frame",null,14,57.4,1,14,805.1,803.6,"2376*1100*560",{"v":1.463616,"d":"1.46"},{"v":1.463616,"d":"1.46"},805.1]
["8","竖向支撑架TR Vertical Frame",null,12,37,1,12,445,444,"1776*585*560",{"v":0.5818175999999999,"d":"0.58"},{"v":0.5818175999999999,"d":"0.58"},{"v":445,"d":"445.0"}]
["9","抗风拉杆 Sway Brace",null,14,43,1,14,619,602,"5076*270*430",{"v":0.5893236,"d":"0.59"},{"v":0.5893236,"d":"0.59"},{"v":619,"d":"619.0"}]
["10","竖向风构 Vertical Brace",null,14,15,1,14,210.5,210,"3001*270*180",{"v":0.1458486,"d":"0.15"},{"v":0.1458486,"d":"0.15"},210.5]
["11~12","阴头端柱Post-End-Female",null,4,89,2,2,343.5,332,"2629*432*390",{"v":0.44293392000000004,"d":"0.44"},{"v":0.8858678400000001,"d":"0.89"},{"v":687,"d":"687.00"}]
[null,"阳头端柱Post-End-Male",null,4,77,null,2]
["13~16","桥面板166 Deck-166",null,28,395,4,7,2771.3,2765,"3040*1162*1050",{"v":3.709104,"d":"3.71"},{"v":14.836416,"d":"14.84"},{"v":11085.2,"d":"11085.20"}]
["17","路缘 Kerb",null,14,26,1,14,384.8,364,"3040*536*365",{"v":0.5947456000000001,"d":"0.59"},{"v":0.5947456000000001,"d":"0.59"},{"v":384.8,"d":"384.80"}]
["18","加隙板4.2m Deck Eob Filler4.2m",null,2,85,1,2,171.3,170,"4200*332*97",{"v":0.1352568,"d":"0.14"},{"v":0.1352568,"d":"0.14"},{"v":171.3,"d":"171.30"}]
[]
["1座21.336米桥装箱件清单（总计2座）"]
[]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
[19,"桁架销 Penal Pin",null,67,3,1,67,864.2999999999998,744.2999999999998,"1280*880*1000",{"v":1.1264,"d":"1.13"},{"v":1.1264,"d":"1.13"},{"v":864.2999999999998,"d":"864.3"}]
[null,"保险卡环 Safety Pin",null,67,0.03,null,67]
[null,"联系梁TR Tie Beam",null,4,5.3,null,4]
[null,"支座  Bearing",null,8,13.4,null,8]
[null,"支座板 Baseplate",null,8,13,null,8]
[null,"加隙板螺栓Deck Eob Filler Bolt",null,17,0.35,null,17]
[null,"弦杆螺栓Chord  Reinforcement  Bolt",null,13,0.98,null,13]
[null,"撑架螺栓 Brace Bolt",null,151,0.5,null,151]
[null,"螺纹板 Nut-Deck-Clamp",null,134,0.35,null,134]
[null,"横梁螺栓Transom Bolt",null,34,0.8,null,34]
[null,"地脚螺栓 螺母 平垫圈 Bastplate Bolt",null,17,2,null,17]
[null,"拉杆螺栓Swaybrace Bolt",null,29,0.6,null,29]
[null,"风构螺栓Vertical Brace Bolt",null,44,0.5,null,44]
[null,"螺母M24 NutM24",null,271,"/",null,271]
[null,"螺母M20 NutM20",null,74,"/",null,74]
[null,"弹垫20  Washer",null,135,"/",null,135]
[null,"桥面板螺栓 Deck Screw",null,118,0.35,null,118]
[null,"路缘螺栓 Kerb-Bolt",null,74,0.35,null,74]
[]
[{"$nulls":10},"单桥总重量",null,{"v":28264.359999999997,"d":"28264.4"}]
[{"$nulls":10},"单桥总体积",null,{"v":55.55763444000001,"d":"55.56"}]

{"sheet":"18","index":3,"n_rows":45,"n_cols":13,"rows_kept":45,"merged":[[0,0,0,12],[1,0,2,0],[1,1,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,8],[1,9,2,9],[1,10,2,10],[3,0,4,0],[3,1,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,9,4,9],[5,1,5,2],[5,3,6,3],[6,1,6,2],[7,1,8,2],[7,3,8,3],[7,4,8,4],[7,15,7,16],[7,28,7,29],[7,41,7,42],[7,54,7,55],[7,67,7,68],[7,80,7,81],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,0,14,0],[13,1,13,2],[13,5,14,5],[13,7,14,7],[13,8,14,8],[13,9,14,9],[13,10,14,10],[13,11,14,11],[13,12,14,12],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[19,0,20,12],[21,0,22,0],[21,1,22,2],[21,3,22,3],[21,4,22,4],[21,5,22,5],[21,6,21,8],[21,9,22,9],[21,10,22,10],[23,0,24,0],[23,1,24,2],[23,3,24,3],[23,4,24,4],[23,5,24,5],[23,6,24,6],[23,9,24,9],[25,0,41,0],[25,1,25,2],[25,5,41,5],[25,7,41,7],[25,8,41,8],[25,9,41,9],[25,10,41,10],[25,11,41,11],[25,12,41,12],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2]],"flags":["formulas_cached_only"]}
["1座18.288米桥捆装件清单（总计2座）"]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
["1~2","桁架 Panel-standard",null,24,322,2,5,1613.94,1610,"3163*2350*712",{"v":5.2923316,"d":"5.29"},{"v":10.5846632,"d":"10.58"},{"v":3227.88,"d":"3227.9"}]
["3~4","桁架 Panel-standard",null,null,322,2,7,2257.94,2254,"3163*2350*980",{"v":7.284389,"d":"7.28"},{"v":14.568778,"d":"14.57"},{"v":4515.88,"d":"4515.9"}]
["5","超宽道横梁(6.2米)ExtreTransom-6.2m",null,7,471.3,1,4,1916.2,1885.2,"6200*800*575",{"v":2.8520000000000003,"d":"2.85"},{"v":2.8520000000000003,"d":"2.85"},1916.2]
["6",{"$nulls":4},1,3,1436.9,1413.9,"6200*590*575",{"v":2.10335,"d":"2.10"},{"v":2.10335,"d":"2.10"},1436.9]
["7","水平支撑架TR Bracing Frame",null,12,57.4,1,12,690.3,688.8,"2376*925*560",{"v":1.230768,"d":"1.23"},{"v":1.230768,"d":"1.23"},690.3]
["8","竖向支撑架TR Vertical Frame",null,10,37,1,10,371,370,"1776*510*560",{"v":0.5072256,"d":"0.51"},{"v":0.5072256,"d":"0.51"},{"v":371,"d":"371.0"}]
["9","抗风拉杆 Sway Brace",null,12,43,1,12,533,516,"5076*250*430",{"v":0.54567,"d":"0.55"},{"v":0.54567,"d":"0.55"},{"v":533,"d":"533.0"}]
["10","竖向风构 Vertical Brace",null,12,15,1,12,180.5,180,"3001*180*180",{"v":0.0972324,"d":"0.10"},{"v":0.0972324,"d":"0.10"},180.5]
["11~12","阴头端柱Post-End-Female",null,4,89,2,2,343.5,332,"2629*432*390",{"v":0.44293392000000004,"d":"0.44"},{"v":0.8858678400000001,"d":"0.89"},{"v":687,"d":"687.00"}]
[null,"阳头端柱Post-End-Male",null,4,77,null,2]
["13~16","桥面板166 Deck-166",null,24,395,4,6,2376.3,2370,"3040*996*1050",{"v":3.179232,"d":"3.18"},{"v":12.716928,"d":"12.72"},{"v":9505.2,"d":"9505.20"}]
["17","路缘 Kerb",null,12,26,1,12,332.8,312,"3040*536*340",{"v":0.5540096000000001,"d":"0.55"},{"v":0.5540096000000001,"d":"0.55"},{"v":332.8,"d":"332.80"}]
["18","加隙板4.2m Deck Eob Filler4.2m",null,2,85,1,2,171.3,170,"4200*332*97",{"v":0.1352568,"d":"0.14"},{"v":0.1352568,"d":"0.14"},{"v":171.3,"d":"171.30"}]
[]
["1座18.288米桥装箱件清单（总计2座）"]
[]
["箱号","构件名称",null,"数量","单件重量","箱数","每箱Each case",null,null,"外形尺寸","单箱体积","小计体积","小计重量"]
[{"$nulls":6},"件数","毛重","净重",null,null,"Total","Total"]
["No.","Name  component",null,"Qty","Kg/piece","Cases","pieces","G.W.","N.W.","Overall Size","Vol. of  ","Volume","Weights"]
[{"$nulls":7},"(Kg)","(Kg)",null,"each  case","(m3)","(Kg)"]
[19,"桁架销 Penal Pin",null,59,3,1,59,792.02,672.02,"1280*880*1000",{"v":1.1264,"d":"1.13"},{"v":1.1264,"d":"1.13"},{"v":792.02,"d":"792.0"}]
[null,"保险卡环 Safety Pin",null,59,0.03,null,59]
[null,"联系梁TR Tie Beam",null,4,5.3,null,4]
[null,"支座  Bearing",null,8,13.4,null,8]
[null,"支座板 Baseplate",null,8,13,null,8]
[null,"加隙板螺栓Deck Eob Filler Bolt",null,17,0.35,null,17]
[null,"撑架螺栓 Brace Bolt",null,130,0.5,null,130]
[null,"螺纹板 Nut-Deck-Clamp",null,118,0.35,null,118]
[null,"横梁螺栓Transom Bolt",null,29,0.8,null,29]
[null,"地脚螺栓 螺母 平垫圈 Bastplate Bolt",null,17,2,null,17]
[null,"拉杆螺栓Swaybrace Bolt",null,25,0.6,null,25]
[null,"风构螺栓Vertical Brace Bolt",null,38,0.5,null,38]
[null,"螺母M24 NutM24",null,222,"/",null,222]
[null,"螺母M20 NutM20",null,63,"/",null,63]
[null,"弹垫20  Washer",null,118,"/",null,118]
[null,"桥面板螺栓 Deck Screw",null,101,0.35,null,101]
[null,"路缘螺栓 Kerb-Bolt",null,63,0.35,null,63]
[]
[{"$nulls":10},"单桥总重量",null,{"v":24359.98,"d":"24360.0"}]
[{"$nulls":10},"单桥总体积",null,{"v":47.90814944,"d":"47.91"}]